{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Packet Time L24, 48kHz"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Packet Time L24, 48kHz","index":0,"n_rows":91,"n_cols":6,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Format (bytes)","Sample rate (kHz)","Packet time (ms)","Channels per stream","Frame size (samples)","Payload (bytes)"]
[3,48,0.125,1,6,18]
[3,48,0.16666666666666666,1,8,24]
[3,48,0.25,1,12,36]
[3,48,0.3333333333333333,1,16,48]
[3,48,0.5,1,24,72]
[3,48,0.6666666666666666,1,32,96]
[3,48,1,1,48,144]
[3,48,1.3333333333333333,1,64,192]
[3,48,2,1,96,288]
[3,48,4,1,192,576]
[3,48,0.125,2,6,36]
[3,48,0.16666666666666666,2,8,48]
[3,48,0.25,2,12,72]
[3,48,0.3333333333333333,2,16,96]
[3,48,0.5,2,24,144]
[3,48,0.6666666666666666,2,32,192]
[3,48,1,2,48,288]
[3,48,1.3333333333333333,2,64,384]
[3,48,2,2,96,576]
[3,48,4,2,192,1152]
[3,48,0.125,4,6,72]
[3,48,0.16666666666666666,4,8,96]
[3,48,0.25,4,12,144]
[3,48,0.3333333333333333,4,16,192]
[3,48,0.5,4,24,288]
[3,48,0.6666666666666666,4,32,384]
[3,48,1,4,48,576]
[3,48,1.3333333333333333,4,64,768]
[3,48,2,4,96,1152]
[3,48,0.125,6,6,108]
[3,48,0.16666666666666666,6,8,144]
[3,48,0.25,6,12,216]
[3,48,0.3333333333333333,6,16,288]
[3,48,0.5,6,24,432]
[3,48,0.6666666666666666,6,32,576]
[3,48,1,6,48,864]
[3,48,1.3333333333333333,6,64,1152]
[3,48,0.125,8,6,144]
[3,48,0.16666666666666666,8,8,192]
[3,48,0.25,8,12,288]
[3,48,0.3333333333333333,8,16,384]
[3,48,0.5,8,24,576]
[3,48,0.6666666666666666,8,32,768]
[3,48,1,8,48,1152]
[3,48,0.125,10,6,180]
[3,48,0.16666666666666666,10,8,240]
[3,48,0.25,10,12,360]
[3,48,0.3333333333333333,10,16,480]
[3,48,0.5,10,24,720]
[3,48,0.6666666666666666,10,32,960]
[3,48,1,10,48,1440]
[3,48,0.125,12,6,216]
[3,48,0.16666666666666666,12,8,288]
[3,48,0.25,12,12,432]
[3,48,0.3333333333333333,12,16,576]
[3,48,0.5,12,24,864]
[3,48,0.6666666666666666,12,32,1152]
[3,48,0.125,16,6,288]
[3,48,0.16666666666666666,16,8,384]
[3,48,0.25,16,12,576]
[3,48,0.3333333333333333,16,16,768]
[3,48,0.5,16,24,1152]
[3,48,0.125,20,6,360]
[3,48,0.16666666666666666,20,8,480]
[3,48,0.25,20,12,720]
[3,48,0.3333333333333333,20,16,960]
[3,48,0.5,20,24,1440]
[3,48,0.125,24,6,432]
[3,48,0.16666666666666666,24,8,576]
[3,48,0.25,24,12,864]
[3,48,0.3333333333333333,24,16,1152]
[3,48,0.125,30,6,540]
[3,48,0.16666666666666666,30,8,720]
[3,48,0.25,30,12,1080]
[3,48,0.3333333333333333,30,16,1440]
[3,48,0.125,32,6,576]
[3,48,0.16666666666666666,32,8,768]
[3,48,0.25,32,12,1152]
[3,48,0.125,40,6,720]
[3,48,0.16666666666666666,40,8,960]
[3,48,0.25,40,12,1440]
[3,48,0.125,48,6,864]
[3,48,0.16666666666666666,48,8,1152]
[3,48,0.125,64,6,1152]
[]
["Format L24: 24 bit or 3 bytes per audio sample"]
["Channels per stream: commonly used numbers, other combinations are possible"]
["Frame size: possible combination for 52-7067A TX setup"]
["The frame size defines the number of audio samples per channel per network packet."]
["Payload: Ethernet packet payload, max. 1440 bytes"]